
Manual gear reducers



In 2015, **ENGRENAGES HPC** has completed its range of gear reducers by adding several manually operated versions.

**This part of the range now comprises:**

* Manually operated right angled gear reducers with ratios from 1:1 to 30:1
* Manually operated worm and wheel gear reducers with ratios from 1:1 to 23:1

**General Characteristics:**

* Housing in glass fibre reinforced Polyamide PA6 or Zamak (depending on model)
* Maximum torque up to 17Nm (depending on model)

**Accessories:**

* Hexagonal steel drive shaft
* Stainless steel operating handle with hexagonal end and plastic handle

**Application :**

* For any application requiring manual operation